
This File contains som example for input of DGP-Solver
-------------------------------------------------------


Example - 1
2-2 CDPRs
DGP-Solver solves DGP with 1 and 2 active cables  
The adjustment of Bertini is set as default
-------------------------------------------------------

Coordinates Points A: 0,0,0;5,0,-0.5
Coordinates Points B:-1,0,-0.5;1,0,0
Coordinates Point G:0,0,0
Load:0,0,10
Cable Lengths:6.5,6.5
Cable Groups:1,2
NCPUs:1
Method Type:0
CONFIG

-------------------------------------------------------


Example - 2
A 3-3 CDPRs
DGP-Solver solves DGP with 1,2 and 3 active cables 
-------------------------------------------------------

Coordinates Points A: 0,0,0;10,0,0;0,12,0
Coordinates Points B:1,0,0;0,1,0;0,0,1
Coordinates Point G:0,0,0
Load:0,0,10
Cable Lengths:7.5,10,9.5
Cable Groups:1,2,3
NCPUs:2
Method Type:0
CONFIG
MAXNUMBERSTEPS:500;
-------------------------------------------------------


Example - 3
A 4-4 CDPRs
DGP-Solver solves DGP with 1,2,3,4 active cables 
If prameter homotopy continuation misses 10 solutions DGP-Solver switch to general homotopy continuation
-------------------------------------------------------

Coordinates Points A: 0,0,0;9,0,1;11,9,0;-2,8,-1
Coordinates Points B: -2,-1,-1;1,-2,0;2,1,-1;0,2,-1
Coordinates Point G:0,0,0
Load:0,0,1
Cable Lengths:6,7,8,9
Cable Groups:1,2,3,4
NCPUs:2
Method Type: 1
NSolMiss: 10
CONFIG
-------------------------------------------------------


Example - 4
A 5-5 CDPRs
DGP-Solver solves DGP with 2 and 5 active cables 
If prameter homotopy continuation misses 10 solutions DGP-Solver switch to general homotopy continuation
-------------------------------------------------------

Coordinates Points A: 0,0,0;1,2,-0.75;3.5,1,1;3.25,-1,1;1,-2,-0.5
Coordinates Points B: -1,0,-1;-0.5,1,-1.25;0.75,0.75,-1.25;0.5,-0.75,-1.25;-0.25,-0.8,-1.5
Coordinates Point G:0,0,0
Load:0,0,10
Cable Lengths:4.5,5,3,3.75,4.75
Cable Groups:2,5
NCPUs:2
Method Type: 1
NSolMiss: 10
CONFIG
MAXNUMBERSTEPS:500;






